**MEMORY :**   
INSTALLED SIZE : 8 GB   
MAXIMUM SIZE : 192 GB   
TECHNOLOGY : DDR3 SDRAM   
MEMORY SPEED : 1600 MHZ   
MEMORY SPECIFICATION COMPLIANCE : PC3L-12800R   
FORM FACTOR : LRDIMM 240-PIN   
FEATURES : REGISTERED, LOW-VOLTAGE   
CONFIGURATION FEATURES : 1 X 8 GB   
RAM SUPPORTED :   
PC3-10600 - 384 GB - LOW VOLTAGE - LOAD-REDUCED   
PC3-12800 - 192 GB - REGISTERED   
PC3-10600 - 96 GB - LOW VOLTAGE - UNBUFFERED - ECC   
PC3-10600 - 192 GB - LOW VOLTAGE - REGISTERED   
PC3-12800 - 96 GB - UNBUFFERED - ECC   
  
**STORAGE & STORAGE CONTROLLER :**   
STORAGE HARD DRIVE : NONE SHIP STANDARD, INCLUDES 8 SFF HARD DRIVE BLANKS   
INTERNAL STORAGE : 8 SFF HDD BAYS   
STORAGE CONTROLLER TYPE : 1 X SATA - INTEGRATED - PCI EXPRESS 2.0 X4   
CONTROLLER INTERFACE TYPE : SATA 6GB/S / SAS 6GB/S   
STORAGE CONTROLLER NAME : HP DYNAMIC SMART ARRAY B320I   
CHANNEL QTY : 8   
RAID LEVEL : RAID 0, RAID 1, RAID 10   
BUFFER SIZE : 512 MB

Type of info for the patients: picture, x-ray, lab reports,